# **Quick Start**

1. Turn on ASMO
2. Wait until the LED turns green
3. Connect to ASMOs wifi:  
   SSID: asmo  
   Pass: 12345678
4. Navigate to <http://10.0.0.1:8080>

# **Troubleshooting**

If the LED turns red for 5 seconds and then goes off:

1. Connect to ASMOs wifi
2. Connect to 10.0.0.1 via ssh  
   User: pi  
   Pass: raspberry
3. sudo systemctl start AsmoAPI
4. sudo systemctl status AsmoAPI -l

This will output the messages from ASMOs Software.  
Alternatively, run the webserver directly:  
cd /home/pi/Asmo/AsmoApi/AsmoApi  
python AsmoApi.py